# Summary for JJF 1610:2017

A | Add notes button | B | End test button
C | Statistic parameters |  |

The table displays the results of each calibration point of high torque rate reading and low torque rate reading. The available parameters are:

- Target [Nm]: target value of each calibration point of high torque rate and low torque rate.

- X [Nm]: mean value of the acquired measurements of high torque rate and low torque rate.

- Relative tolerance [%]: relative tolerance of high torque rate reading (δH) and low torque rate reading (δL).

- Repeatability [%]: repeatability of high torque rate reading (RH) and low torque rate reading (RL).

- U [%]: expanded uncertainty.

To print the test report: on the upper-right corner of the Summary category, tap Print report.

## Applies to: