# Configuring a TCP/IP connection with STRwrench

1. In the Home page, tap Measuring devices.

2. On the upper-right corner of the Measuring devices page, tap Add.

3. In the Measuring devices type window, tap STRwrench.

   After selecting STRwrench, the Connection category of the Add STRwrench page is automatically displayed.

   The General category is automatically filled once the configuration is completed.

4. In the Connection category, configure the following parameters:

   - Connection type: in the drop-down list select TCP/IP.

   - Device IP address: type the IP address of the STRwrench to be connected.

   - Device port number: type the port number of the STRwrench to be connected.
     Default value is 6688.

   - Trace read: In the drop-down list, select one of the following option for the trace reading from the STRwrench:

     - Always: always read traces.

     - NOK only: read NOK traces only.

     - Never: never read traces.

   - Residual double result: select the check box to save the torque/angle values of both Residual point and Peak point.
     If the check box is not selected, only the torque/angle values of the Residual point are saved.

   - Residual max torque behavior: select the check box to have a Not OK result when the Residual point is within the limits and the Peak point exceeds the maximum torque.
     If the check box is not selected, the result status of the test is OK when the Residual point is within the limits and the Peak point exceeds the maximum torque.

5. On the upper-right corner of the Add STRwrench page, tap Save.

## Applies to: