# Editing Joint inspection

1. In the Joint page, select a joint.

2. In the Edit joint toolbar, tap Inspection.

3. In the Inspections category, tap the inspection to edit.

4. In the Edit inspection page, change the necessary parameters.

5. In the upper-right corner of the Edit inspection page, tap Save.

If the inspection is sent by an external software, it is not possible to edit it.

## Applies to: