# Configuring the SIGOP/SCOUP integration

1. In the Home page, tap Configuration > SIGOP/SCOUP > Configuration.

2. Select the Enabled check box to activate the SIGOP/SCOUP integration.

3. In the Route input file path field, type the path of the file that contains the tests to import.

   If the path typed is relative, the STpad searches the file into the first available device from the Network location and the Devices with Removable Storage.

4. In the Test output file path field, type the path of the file where the results are exported.

   If the path typed is relative, the STpad writes the file into the first available device from the Network location and the Devices with Removable Storage.

5. From the Import inspection as drop-down list select between:

   - Cm/Cmk ISO, to import tests from the route file as Cm/Cmk ISO inspections.

   - SPC, to import tests from the route file as SPC inspections.

   When importing Cm/Cmk ISO inspections, the batch size is taken from global default value(Configuration > Default values > Inspection default values > Number of samples).

   When importing SPC inspections, the batch size is taken from route input file.

6. Select the Ask VIN check box to request the VIN when running an inspection.

7. Tap on the Save button.

## Applies to: