# Label

In the Home page, tap Configuration > General settings > Label.

To configure the label printing, set the following parameters:

General category

- Default printer: select the printer to use for the label printing.
  The supported printers are: Brother PT-P950 NW, Zebra GX 420t, and Toshiba TEC B-EV4.

- Standard size: select the size of the default label to print.
  The available sizes are: 50 x 25, 57 x 25, 68 x 25. All the size are in millimeters.

- Standard orientation: select the orientation of the default label to print.
  The two option are: portrait and landscape.

Inspections category

For each inspection type, select the label template to use from the drop-down menu.

Templates category

To create customized label templates, please contact Atlas Copco Service Personnel.

To import a custom label template:

1. Copy the custom template file on a USB storage device in a subfolder named label_templates.

2. Insert the USB into the USB port of the device.

3. Tap on the Import button and select the file of interest.

To delete a custom label template:

1. Tap on the Select button and select the check box(es) of the label template(s) to delete.

   Label templates that are currently in use cannot be selected and deleted.

2. Tap on the Delete button.

The label can be printed for tool calibrations, Cm/Cmk, SPC, ISO 6789 and VDI-VDE inspections.

The label of tool calibrations displays the following information:

- Tool ID

- Operator

- Last check

- Next check

- Calibration value

The "Next check" indicated in the label is always the expiry date in the event that the test result is OK. The calculation of the "Next check" date is not affected by the test OK or NOK status.

## Applies to: