# Controller parameters

General category

- Name: type the name of the controller. The maximum number of characters is 50.

- Serial number: type the Serial number of the controller. The maximum number of characters is 50.

- Type: select the controller between the following:

  - Power Focus

  - Power MACS

  - Other controller

  - Open Protocol

- Device IP Address: type the IP address of the controller. This parameter is available for controller type Power Focus and Open Protocol.

- Port number: type the port number of the controller. This parameter is available for controller type Power Focus and Open Protocol.

- Baud rate: select the baud rate. This parameter is unavailable for controller type Power MACS.

## Applies to: