# Importing a Raw Trace

This feature allows to import traces from an external software, by importing data from a file.
For information on the file, refer to Requirements for raw traces files

1. On the USB storage device, create a directory and rename it curves.

2. Add the curves to the directory. The file formats supported are .qap and .txt.

3. Insert the USB storage device into the USB port of the device.

4. In the upper-right corner of the Raw category, tap Import.

5. In the Select file dialog box, select the curve to import.

   It is possible to import up to 10 traces. When the maximum number of traces to import is reached, the Import button is disabled.

## Applies to: