# Joint inspections

The available inspection types for the joints are:

- Cp/Cpk ISO

- SPC (joint)

It is possible to save two inspection with the same name and the same target objet.

A warning message is displayed to advise the operator an inspection with the same name already exists.

Select Yes to save the inspection.

Select No not to save the inspection.

In this Section

- Adding a Joint inspection
- Cp/Cpk ISO parameters
- SPC (joint) parameters
- Adding a Joint check inspection trough the template file
- Deleting Joint inspection
- Editing Joint inspection
- Running Joint inspection

## Applies to: