# Connected transducer

The following notifications are not available for MT TS transducers.

If the transducer connected to the measuring device is overloaded, a warning message is displayed to inform the operator about the status of the transducer.

When a transducer is used for the first time, an information message is displayed to inform the operator that the first usage date is set to the current date.
Select Yes to set the first usage date to the current date.
Select No not to set the date. If this option is selected, at the next transducer use, the message will be displayed again.

If the transducer calibration is expired, an Information message is displayed to inform the operator that the transducer must be calibrated. It is still possible to use the transducer for testing.

## Applies to: