# Running Tool inspection

1. In the Home page, tap Tool.

2. In the Tool page, tap Play to run the inspection.

3. In the Select transducer dialog box, select the transducer to be used during the Inspection.

4. Run the test.
   During the test, the following page is updated in real time.

   The following screen is displayed only if the Measuring device is set to STbench.

   In the event the STbench has not reached the optimal operating pressure, the message STbench is pressurizing the circuit is displayed. The pop-up message automatically closes when the correct pressure is reached and the test starts.

   A | Inspection categories | B | Tuning brake button
   C | Batch size counter | D | Command buttons
   E | Test values | F | Brake status indicator
   G | Test values summary | H | Variable chart

If you change the speed of the tool under inspection, to collect consistent results you must always tap the Tuning brake button before running a new test, even if the inspection settings have not been modified.

In this Section

- Results category
- Summary category for Cm/Cmk and CAM/Cpk CNOMO
- Summary category for SPC
- Summary for ISO 6789:2003
- Summary for ISO 6789-2:2017
- Summary for ISO 5393
- Summary for VDI/VDE 2465-2
- Summary for JJF 1610:2017
- Torque/angle statistic category
- Trace category

## Applies to: