# Calibrating Power Focus

1. Connect the system (for more information, see STbench Operation Manual / STpad Operation Manual – Operation – Calibrating Power Focus - General Information).

2. Switch on both the device and the Power Focus. On the Power Focus, select the necessary Pset according to customer needs.

   For Power Focus 6000, it is necessary to enable the QA Calibration in the Tool section and select the virtual station linked to the tightening program to use for the calibration.

   For more information about how to select a Pset/Tightening program on the Power Focus, see Power Focus Manual.

3. On the device, configure the Power Focus (for more information, see Controllers).

4. After configuring the Power Focus, configure the tool to calibrate (for more information, see Adding a Tool).

5. After configuring the tool to calibrate, configure the calibration inspection (for more information, see Adding a Calibration inspection).

   At the end of the configuration of the calibration inspection, the following is displayed:

   A | Play

6. Tap Play for running the Inspection.

   If in the Controller category of the calibration inspection, Manual selection is selected, a synchronization mode dialog box appears during the calibration. Select the synchronization mode to continue the calibration process.

   At the end of the calibration inspection, the following is displayed:

   A | Calibration inspection Toolbar

   On the Calibration inspection Toolbar, the Results page shows a plot with all the results of the inspection (on the right side), and the list of the results of the inspection (on the left side).

7. On the Calibration inspection Toolbar, tap Summary to display the following page:

   Tap Save and Exit, then tap Yes in the dialog box that opens to save the new calibration value on the tool calibrated.

If during the calibration process the internet connection is unstable, a dialog box is displayed. Then, it is possible to insert the controller result manually.

If a label printer is configured, a dialog box asking to confirm the printing of the label is displayed.

## Applies to: