# Running a forced by inspection route

1. Connect the device to the necessary measuring device (for more information, see “Measuring devices”).

2. Import the necessary route(s) with "Forced by inspection" sequence on the device (for more information, see “Adding Route(s) through the Template file”).

3. In the Route page, tap Play in correspondence of the enabled inspection.

In this Section

- Navigating a forced by inspection route

## Applies to: