# Installing Atlas Copco Data Communication

The DataCommunication Installation Configurator helps configure the necessary settings before starting the Atlas Copco Data Communication service.

1. Double-click or run the AtlasCopco Data Communication-x.x.x.msi file.

2. In the InstallShield Wizard, read the information and click Next.

3. Read and accept the terms in the License Agreement and click Next to continue.

   The Destination Folder window opens.

4. Click Change... to choose a different location to install the configurator. The default installation location is C:\Program Files (x86)\Atlas Copco\. The Ready to Install the Program window opens.

5. Click Install to begin the installation. After the installation is complete, the InstallShield Wizard Completed window opens.

6. Click Finish to open the DataCommunication Installation Configurator.

   The DataCommunication Installation Configurator opens.

7. Continue the configuration of the Atlas Copco Data Communication service by going to Working with the DataCommunication Installation Configurator.

Relevant Information

- Troubleshooting During Installation

In this Section

- Default Databases