# Trace View Tab - Flow Drill Fastening

The Trace view tab opens up when selected from the result list, generated from the Reports tab centers.

The trace view displays detailed joint analysis, using data measured for different parameters like Torque, Joining Unit Force, Penetration Depth, Normal/Actual Speed, Overlap and Main Cylinder Stroke etc.

Trace results are only available if trace results are sent out from the controller.

The trace can be selected and displayed with the X-axis representing time, while two Y-axes show values based on options chosen from dropdown menus.

When working and analyzing the trace it is possible to do the following:

- Hover on the trace to view further detailed data.

- Draw a box in a specific area to zoom in.

- Select and hold the Shift key and drag, to pan or zoom an area. See Microvideo.

- Select Reset zoom to go back to the original view.

- Select the More icon to Print or Export the trace details.

- Select or deselect a trace from the list to view or hide the trace.

- Select one of the trace curves to open the Magnified view of graphs.

View further details in the table below the trace:

- General

- Torque

- Angle

## Microvideo

How to use the trace zoom and pan function
Relevant Information

- Exporting or Printing the Trace View