# Trace View Tab - Tightening and Riveting

The Trace view tab opens up when selected from the result list, generated from the Reports tab centers.

The trace view displays detailed joint analysis, using data from measured torque and angle values for a specific rundown. The information is either shown as a data table, or a combined chart and data table.

Trace results are only available if trace results are sent out from the controller.

The following traces can be selected and viewed:

- Torque/Angle

- Torque/Time

- Angle/Time

- Speed/Time

- Current/Time

- Boxplot: Torque

- Boxplot: Angle

Boxplot: Torque and Boxplot: Angle options are displayed only for MicroTorque controller.

Traces for MicroTorque and PF6000 display optional trace data in Torque/Angle, depending on the controller settings.

Seating point in trace:

- Rundown complete

- First torque

- Final torque

When working and analyzing the trace it is possible to do the following:

- Hover on the trace to view further detailed data.

- Draw a box in a specific area to zoom in.

- Select and hold the shift key and drag, to pan or zoom an area. See Microvideo.

- Select Reset zoom to go back to the original view.

- Select the more icon to Print or Export the trace details.

- Select or deselect a trace from the list displayed to view or hide the trace.

- Use Sync traces - synchronize and compare the traces in an easy way. It is possible to select different sync values for example, Peak, Rundown Complete, First Target or Custom value.

- Select one of the trace curves to open the Magnified view of graphs.

- Select a specific step from a multi-step result, it will display that part of the graph and information belonging to that step in the area below for Torque and Angle traces.

- Toggle step limit boxes on and off.

View further details in the table below the trace:

- General

- Torque

- Angle

## Microvideo

How to use the trace zoom and pan function
Relevant Information

- Exporting or Printing the Trace View
- Synchronizing Traces