# Tools with accessories

1. Thread the circlip and the yoke ring onto the tool.

2. Attach the rubber cover onto the motor cover.

3. Attach the clamp rings on the rubber cover.

   NOTICE

   Make sure the clamp rings are oriented with the flange according to the picture.

4. Hold the tool using a vise and assembly/disassembly tool against the rubber cover.

5. Push the yoke ring onto the clamp rings.

6. Secure the yoke ring with a circlip in the slot of the clamp rings.