# For torque less than 100 Nm

- The clamping area shall be as large as possible

Avoid clamping on the angle head and cap nut.

STB/ST/ES/SL/SR equipment:

- Fit the clamp around the motor.

- Clamp on the sides of the tool.

STR equipment:

- Preferably, choose a solution that Atlas Copco provides.

- If not possible, fit the clamp around the motor. Cover the inside of the clamp using a rubber cloth to protect the marking plates and plastic cover of the motor.

- Clamp on the top and bottom of the tool.

- Keep the clamping load as low as possible.