# Tools up to 50 Nm

1. Hold the tool using a vise and assembly/disassembly tool.

2. Attach the rubber cover onto the motor cover next to the assembly/disassembly tool.

3. Attach the clamp rings on the rubber cover.

   NOTICE

   Make sure the clamp rings are oriented with the flange according to the picture.

4. Attach the yoke ring to the tool by pushing it onto the clamp rings.

   NOTICE

   Make sure the yoke is pointing to the front end of the tool.

5. Secure the yoke ring with a circlip in the slot of the clamp rings.