# Tools with scanner accessory

1. Attach the rubber cover on the motor cover of the tool.

2. Attach the clamp rings on the rubber cover.

   NOTICE

   Make sure the clamp rings are oriented with the flange facing the scanner.

3. Attach the yoke ring to the tool by pushing it onto the clamp rings.

   NOTICE

   Make sure the rubber cover and the clamp rings are aligned.

4. Secure the yoke ring with a circlip in the slot of the clamp rings.