# Customer-developed fixturing equipment

- The guidelines differ depending on the separate torque ranges for the tools, and if the tool is equipped with a Torque Multiplier.

- Never put a clamp holding the fixture on the surface covering the torque transducer!

- Avoid point loads.

- Clamping load must not exceed 2 kN.

There are no restrictions on the following:

- Materials used for the clamps

- Bearing or swiveling arrangement for the fixture

- Overall thickness of the clamp

In this Section

- For all tools equipped with a Torque Multiplier
- For torque less than 100 Nm
- For torque between 100 and 200 Nm
- For torque above 200 Nm