# Changing the air inlet adapter

All PFD1500 tools will be delivered with NPT air inlet adapter as standard. Additional BSP air inlet adapter will be included in the box together with the tool on delivery.

WARNING

Make sure that the air supply is not connected.

CAUTION

Wear gloves to avoid personal injury because of sharp cutting edges. Only experienced maintenance personnel can assemble or disassemble the product.

Required tools

- Vise

- Spanner

1. Remove the adapter.

   Make sure that the filter is still in place.

2. Replace the adapter with the new one (included in the box). Move the o-ring from the old adapter to the new one.

3. Put the adapter back in original position. Tighten the adapter.

   Make sure that the filter is in position.