# Range gear

Total amount of lubrication: 15 ml.

Turn gear while lubricating at least two turns.

Ensure that gear is running normally without hacking.

Pos | Description
--- | ---
A1 | Ensure that the outside and sliding surface of the radial seals are lubricate with lubricant A before assembly.
A2 | Ensure that needle bearings are completely filled with lubricant A.
A3 | Ensure that the O-rings are well greased with lubricant A.