# Assembling Indexer

Perform the following steps to assemble the indexer or moving it to another tool:

1. Loosen the nut that connects the indexer to the tool's head.

2. Clean the thread of the nut from glue.

3. Check the splines on the lower part that is attached to the front part of the indexer for damage. Clean off any glue.

4. Check the splines on the lock pin on the indexer's upper housing for damage and clean off any glue. As the indexer is parted, push the button to ensure that the lock pin on the indexer runs smoothly in and out of the housing.

5. Replace the part or complete indexer if there is any damage to the indexer's part.