# Motor valve

| Drill bit/Material | Drill bit/Material | Drill bit/Material
--- | --- | --- | ---
| <1/2" Titan/Alu | <3/4" Titan/Alu | <1 1/4" Titan/Alu
Cycles | (Use kit, Ordering No.) | (Use kit, Ordering No.) | (Use kit, Ordering No.)
Every day | Test function* | Test function* | Test function*
Every 1000 drilled holes |  |  |
Every 3000 drilled holes |  |  |
Every 6000 drilled holes |  |  |
Every 12000 drilled holes |  |  |
Every 24000 drilled holes | 4141 0102 91 | 4141 0102 91 | 4141 0102 91
Every 48000 drilled holes |  |  |

* Emergency stop.