# Installing the ChipLet

WARNING

Make sure that the air supply is not connected.

CAUTION

Wear gloves to avoid personal injury because of sharp cutting edges. Only experienced maintenance personnel can assemble or disassemble the product.

Required tools

- Vise

- Torx screwdriver

- Allen key

- Mounting tool

Prerequisites

Before installing the ChipLet, make sure that the following components are removed:

- Front part

- Drill bit

- Spindle

- Spindle guard

1. Fasten the drill in a vise.

2. Remove the screw and the feed cassette cover.

3. Remove the four screws with the two washers and the feed cassette.

4. Remove the depth position valve.

5. Remove the two screws and the cap.

6. Remove the thrust washer.

7. Put the chiplet with the o-ring in position. A click sound is heard when the chiplet is in position.

8. Fasten the chiplet with two screws and tighten them to 8 Nm.

9. Put the depth position valve back in position, fasten it and tighten to 1 Nm.

10. Put the feed cassette back in position and fasten the four screws and two washers to 8 Nm.

11. Put the cassette cover back in position on the cassette and fasten it with one screw to 3 Nm.