# Installing the torque arm

The tool torque should not exceed the specified torque range of each specific arm.

Do not use SMC 200 and SMC 300 with a bench stand.

Mounting on a bench

- Find the optimal position for the operator to handle the torque arm.

- Install the torque arm straight in front of the operator or alternatively to the left or right depending on whether the operator is left or right-handed.

- Firmly tighten the screws in the holder that connects the torque arm to the bench stand. The bench stand is pre-drilled for fixing to a bench.

- Attach the safety wire (see Spare Parts) to a second point that does not limit the working area.

Mounting on a ceiling

- Put the mounting point straight above, or as close as possible to, the point where the torque is applied.

- Make sure that the fixation point can handle the weight and the torque of the chosen torque arm.

- Attach the safety wire (see Spare Parts) to a second point that does not limit the working area.