# Setting of tightening torque

The adjusting screw is accessible through the hole in the housing. If necessary, turn the outgoing spindle.

After adjusting, it is important to remember to assemble the plug of the hole in the housing.

It is recommended to start at min. torque setting - when the adjustment screw is screwed out approx. 6 turns from the bottom position. Do not screw out any further.

When using the machine above recommended maximum torque it might result in improper function and faster wear. Always check the setting on your actual joint.