# Technical data for QST Nutrunners

Ordering No | 8435606020
Model | QST62-150COT-T50-L152-H13
Gear ratio | 13.94
Min C-C | 45
Socket holder size | 1/2 in
Sound power | dB(A)
Sound pressure | <70 dB(A)
Sound standard | ISO15744
Sound uncertainty | dB(A)
Speed | 450 r/min
Torque range | 30–150 Nm
Torque range | 22–110 ft lb
Travel | 50 mm
Weight | 12.8 kg, 28.2 lb
A | 152.5mm
B | mm
C | mm
D | mm
E | 586mm

- CT - Straight Nutrunner

- COT - Offset Nutrunner

- CTV - Angle head Nutrunner