# Multi Charger

## Charger

# Product Information

# General Information

WARNING

Risk of Property Damage or Severe Injury

Ensure that you read, understand and follow all instructions before operating the tool. Failure to follow all the instructions may result in electric shock, fire, property damage and/or severe bodily injury.

- Read all Safety Information delivered together with the different parts of the system.

- Read all Product Instructions for installation, operation and maintenance of the different parts of the system.

- Read all locally legislated safety regulations regarding the system and parts thereof.

- Save all Safety Information and instructions for future reference.

In this Section

- Safety Signal Words
- Warranty
- Website
- ServAid
- Safety Data Sheets MSDS/SDS
- Country of Origin
- Dimensional Drawings

# Safety Signal Words

The safety signal words Danger, Warning, Caution, and Notice have the following meanings:

DANGER | DANGER indicates a hazardous situation which, if not avoided, will result in death or serious injury.
WARNING | WARNING indicates a hazardous situation which, if not avoided, could result in death or serious injury.
CAUTION | CAUTION, used with the safety alert symbol, indicates a hazardous situation which, if not avoided, could result in minor or moderate injury.
NOTICE | NOTICE is used to address practices not related to personal injury.

# Warranty

- Product warranty will expire in 12+1 months after dispatch from Atlas Copco's Distribution Center.

- Normal wear and tear on parts is not included within the warranty.

  - Normal wear and tear is that which requires a part change or other adjustment/overhaul during standard tool maintenance typical for that period (expressed in time, operation hours or otherwise).

- The product warranty relies on the correct use, maintenance, and repair of the tool and its component parts.

- Damage to parts that occurs as a result of inadequate maintenance or performed by parties other than Atlas Copco or their Certified Service Partners during the warranty period is not covered by the warranty.

- To avoid damage or destruction of tool parts, service the tool according to the recommended maintenance schedules and follow the correct instructions.

- Warranty repairs are performed only in Atlas Copco workshops or by Certified Service Partners.

Atlas Copco offers extended warranty and state-of-the-art preventive maintenance through its ToolCover contracts. For further information, contact your local Service representative.

For electrical motors:

- Warranty will apply, only when the electric motor has not been opened.

# Website

Information concerning our Products, Accessories, Spare Parts and Published Matters can be found on the Atlas Copco website.

Please visit: www.atlascopco.com.

# ServAid

ServAid is a portal that is continuously updated and contains Technical Information, such as:

- Regulatory and Safety Information

- Technical Data

- Installation, Operation and Service Instructions

- Spare Parts Lists

- Accessories

- Dimensional Drawings

Please visit: https://servaid.atlascopco.com.

For further Technical Information, please contact your local Atlas Copco representative.

# Safety Data Sheets MSDS/SDS

The Safety Data Sheets describe the chemical products sold by Atlas Copco.

Please consult the Atlas Copco website for more information www.atlascopco.com/sds.

# Country of Origin

For the Country of Origin, please refer to the information on the product label.

# Dimensional Drawings

Dimensional Drawings can be found either in the Dimensional Drawings Archive, or on ServAid.

Please visit: https://webbox.atlascopco.com/webbox/dimdrw or https://servaid.atlascopco.com.

# Overview

# Product Functionality

Position | Description
--- | ---
1 | Battery Holder
2 | Power Cable
3 | LED Green
4 | LED Red

LED Color | LED Behavior | Status | Description
--- | --- | --- | ---
Green | Flashing at 5-second intervals. | Charger idle | The charger is turned on, but no battery is detected.
Green | Flashing at 1-second intervals. | Charging battery | The battery is being charged.
Green | Steady light. | Charging battery | The battery is fully charged.
Red | Steady light. | Error | The battery is too hot or too cold.
Red | Flashing at 1-second intervals. | Error | There is a connection problem or the battery is defective.

# Operation

# Operating Instructions

# Operating the Multi Charger

The mains voltage must match the voltage stated on the type plate of the charger.

1. Connect the charger to the mains power.

   The charger conducts a self-test. Both LEDs glow for one second. The charger then enters standby mode. The red LED turns off, and the green LED starts to flash at 5-second intervals.

2. Slide the battery on the battery holder of the charger. Charging starts automatically and the green LED flashes. The charging time depends on the battery's charge level, capacity, and temperature.

   When the battery is fully charged, the green LED glows. The charger automatically switches to retention charging.

New batteries reach their full capacity after approximately five charging/discharging cycles. Recharge batteries if they have not been used for a long time. The performance of the battery reduces when temperature falls below –10°C. Storing a battery for a long time at temperatures above 40°C can reduce the capacity.

## Sleep Mode

If a battery is completely drained, it will go into sleep mode.

Wake up the battery by doing the following:

1. Insert the battery in the charger.

   The charger will automatically detect that the battery is in sleep mode. The red and green LEDs of the charger start to flash, indicating that wake-up mode is activated.

2. When the charger stops flashing, remove and reattach the battery immediately.

   The charger will resume with the regular charging procedure.

# Troubleshooting

LED Color | LED Behavior | Cause | Solution
--- | --- | --- | ---
Red | Steady light. | The battery is too hot or too cold. | The charging process starts when the battery has reached the correct charging temperature. Refer to the Safety Information of the battery for charging temperatures.
Red | Flashing at 1-second intervals. | The battery has not been placed correctly on the battery holder. | Make sure that the battery is placed correctly on the battery holder.
Red | Flashing at 1-second intervals. | The battery is defective. | Refer to the Product Instruction of the battery for more details on battery LED indicators. If a solution cannot be found in the Product Instruction of the battery, please contact your local Atlas Copco Customer Center for assistance.
Green | Flashing at 5-second intervals. | The battery is fully charged and has automatically shut off as a safety measure.* | The battery can be used as normal.
Green | Flashing at 5-second intervals. | An error has occurred and the battery has been shut off. | Press the release button to start the battery again. If the error occurs again, please refer to the Product Instruction of the battery for more details on battery LED indicators. If a solution cannot be found in the Product Instruction of the battery, please contact your local Atlas Copco Customer Center for assistance.

* This battery behavior was introduced in battery software version 1.6.14.

# Recycling

# Environmental Regulations

When a product has served its purpose it has to be recycled properly. Dismantle the product and recycle the components in accordance with local legislation.

Batteries shall be taken care of by your national battery recovery organization.