# Inspection of Motor Parts

- (R) To be replaced (from Service kit Ordering No. ) at every overhaul.

- End plates: Check that they not are scored or scratched. If these are shallow, polish with fine grinding paste against a face plate. Clean thoroughly.

- Rotor: Check that the end faces do not have any marks or burrs. Check that the splines are not worn or cracked.

- Cylinder: Check that the bore is not scored or scratched. If these are shallow, polish with a fine grinding cloth.