# Setting of the Tightening Torque

To use the tool at a higher torque than recommended maximum torque may result in incorrect function and faster wear.

Always do a control of the tightening torque on the actual joint.

1. Remove the slotted cover plug at the front of the tool.

2. Turn the pulse unit until you see the adjusting screw in the hole.

3. Start at a low torque and increase it until you reach the wanted torque level.