# Initial Setting of Torque

To minimize the risk of damage to the actual joint we recommend to set the torque slightly lower on the test joint than the torque wanted for the application. Make sure to use the same equipment, such as for example extensions, sockets and air pressure on the test joint as will be used on the actual joint.

A | Torque transducer IRTT
B | Test joint
C | ST Analyzer

Make sure to always verify the torque settings on your actual joint.