# Technical Data

Ordering No | 8411101127
Model | LZL25-L-P-AC
Air consumption at 3000 RPM | l/s
Air consumption at 3000 RPM | cfm
Air consumption at max output | 86 l/s
Air consumption at max output | 182 cfm
External parts material | Powder coated cast iron
Free speed | 5800 r/min
Inlet hose | 32 mm
Inlet hose | 1.25 in
Max allowed speed | r/min
Max ambient temperature | 40 ºC
Max output | 3.4 kW
Max output | 4.6 hp
Max radial load at max output | N
Min starting torque | 18 Nm
Min starting torque | 13.2 ft lb
Mounting arrangement |
Outlet hose | 32 mm
Outlet hose | 1.25 in
Power at 3000 RPM | kW
Power at 3000 RPM | hp
Ratio |
Rotation direction | Reversible
Shaft loading code |
Speed at max output | 2800 r/min
Stall torque | 23 Nm
Stall torque | 17 ft lb
Torque at max output | 11.6 Nm
Torque at max output | 8.5 ft lb
Vane type | Lubrication free
Weight | 11.3 kg
Weight | 24.9 lb