# Technical data for QST Nutrunners

Ordering No | 8435606510
Model | QST62-230CT-T50-L152-H19
Gear ratio | 19.04
Min C-C | 63
Socket holder size | 3/4 in
Sound power | dB(A)
Sound pressure | <70 dB(A)
Sound standard | ISO15744
Sound uncertainty | dB(A)
Speed | 330 r/min
Torque range | 40–230 Nm
Torque range | 29–170 ft lb
Travel | 50 mm
Weight | 10.2 kg, 22.5 lb
A | 152mm
B | 25mm
C | 517mm
D | 15mm
E | mm

- CT - Straight Nutrunner

- COT - Offset Nutrunner

- CTV - Angle head Nutrunner