# Lubrication of roller screw

Always read and follow the instruction Preparing for the Lubrication.

Lubricants
Lubricant | Description
--- | ---
Klüberlub® BE 71-501 | http://www.klueber.com/en/product-detail/id/404/

NOTICE

Only use Klüberlub® BE 71-501

Use of other lubricants will permanently damage the press.

NOTICE

Always clean the press on the outside using a lint-free cloth before dismantling.

1. Remove the cover and wipe off grease from the inside using paper or a cloth.

2. Add enough grease to fill the threads evenly onto the visible part of the roller screw.

3. Reassemble the cover.