# Horizontal installation

NOTICE

Radial force on the PST Press piston rod may completely damage the Press.

If the piston rod is not supported enough to withstand radial movements, the piston rod may be completely damaged or the service life and PST Press accuracy will be reduced.

- For vertical installation: Assemble the press vertical on the end surface to prevent radial movement.

- For horizontal installation: Use a radial support in order to keep the piston rod level.

NOTICE

Only support the press on the gray area

Tool weight and support
Press | Tool weight max. (A) | Press support need (B)
--- | --- | ---
PST 5 | 2 Kg | No
PST 10 | 2 Kg | No
PST 20 | 4 Kg | Yes (CBUL only)
PST 35 | 7 Kg | Yes
PST 50 | 10 Kg | Yes
PST 55 | 10 Kg | Yes
PST 100 | 20 Kg | Yes