# Installation overview

The PST press can be installed by the use of the front screw holes or the rear screw holes. See the dimensional drawings on ServAid for installation dimensions.

WARNING

Crushing Hazard

Make sure to stand at a safe distance from the load! A rotating or falling load can cause severe bodily injury or death.

- Always use the fitted lifting eye

- The press weight is 17.5 Kg/39 Ib.

NOTICE

Do NOT use both front and rear installation at the same time.

If the press is mounted both in the front and in the rear, the service life and PST Press accuracy will be reduced.

Lubricants
Lubricant | Description
--- | ---
Klüberlub® BE 71-501 | http://www.klueber.com/en/product-detail/id/404/

NOTICE

Only use Klüberlub® BE 71-501

Use of other lubricants will permanently damage the press.

Torque table
Screw | Torque [Nm] | Torque [ft·lb]
--- | --- | ---
M3 | 1,7 | 1,25
M4 | 4,0 | 2,95
M5 | 7,5 | 5,53
M6 | 13 | 9,59
M8 | 30 | 22,13
M10 | 60 | 44,25
M12 | 110 | 81,13
M14 | 180 | 133
M16 | 280 | 206,52

Oil the threaded parts of the screw before tightening.

Only use screws with strength class 12.9 (DIN 912).