# Disassembling the gearbox

Required tools

- Allen keys or bits 4-10 mm

- Screw bits and sockets

- Torx® keys or bits T6-T25

- Torque wrench

- Lifting device

- Screwdrivers

- Pliers

- Bearing puller (optional)

- Feeler gauge

Lubricants
Lubricant | Description
--- | ---
Klüberlub® BE 71-501 | http://www.klueber.com/en/product-detail/id/404/

NOTICE

Only use Klüberlub® BE 71-501

Use of other lubricants will permanently damage the press.

1. Remove the screws holding the connector cover.

2. Disassemble the connector cover.

3. Disconnect the load cell cable from the motor cable.

4. Fix the press over the gear box in a vice using soft jaws.

5. Disassemble the brake pic. 2-3 (CBUL press only).

6. Unscrew the top cover screws.

7. Remove the top cover by screwing long screws through the threaded holes.

   Remember the position of the guide rings and the preload washers. The preload washers can be placed in the top cover.

8. Disassemble the guide rings and the preload washers.

9. Disassemble the gear wheels, axis and bearings.

10. Disassemble all bearings (x6) using a bearing puller (pic. 10-11).