# Changing the roller bearings

Required tools

- Allen keys or bits 4-10 mm

- Screw bits and sockets

- Torx® keys or bits T6-T25

- Torque wrench

- Lifting device

- Screwdrivers

- Pliers

- Bearing puller (optional)

- Feeler gauge

Lubricants
Lubricant | Description
--- | ---
Klüberlub® BE 71-501 | http://www.klueber.com/en/product-detail/id/404/

NOTICE

Only use Klüberlub® BE 71-501

Use of other lubricants will permanently damage the press.

1. Place the press on a horizontal surface.

2. Disassemble all the screw housing cover screws.

3. Disassemble the screw housing cover.

4. Disassemble the guide rollers and the shim (3x).

5. Disassemble the roller bearings (3x).

   Discard the used roller bearings.

6. Assemble the new roller bearings (3x).

   Apply a thin layer of grease (Klüberlub® BE 71-501) on all parts.

7. Assemble the guide rollers and the shim (3x)

   Apply a thin layer of grease (Klüberlub® BE 71-501) on all parts.

8. Assemble the screw housing cover using the screws.