# Assembling the gearbox

Required tools

- Allen keys or bits 4-10 mm

- Screw bits and sockets

- Torx® keys or bits T6-T25

- Torque wrench

- Lifting device

- Screwdrivers

- Pliers

- Bearing puller (optional)

- Feeler gauge

Lubricants
Lubricant | Description
--- | ---
Klüberlub® BE 71-501 | http://www.klueber.com/en/product-detail/id/404/

NOTICE

Only use Klüberlub® BE 71-501

Use of other lubricants will permanently damage the press.

Required spare parts

- Bearings (x6)

NOTICE

Add a small amount of grease to all surfaces at reassembly.

1. Assemble the bearings on both sides using a press and support (x6).

   Only press and support on the bearing inner rings.

   Apply a thin layer of grease (Klüberlub® BE 71-501).

2. Assemble the guide rings.

3. Assemble the preload washers into the top cover.

4. Assemble the top cover using new screws.

   Tighten the screws crosswise, first to 50% torque, then to 100% torque. Torque according to Installation overview.

5. Assemble the brake pic. 6-7 (CBUL press only).