# Vertical installation front mounting

NOTICE

Do not let the press piston rod support the press weight during service or repairs.

Axial force on the PST press piston rod may completely damage the load cell.

Press | Front mounted
--- | ---
PST 5 | M8 (4x)
PST10 | M8 (4x)
PST20 | M8 (8x)
PST35 | M10 (8x)
PST50 | M10 (8x)
PST60 | M10 (8x)
PST100 | M12 (8x)

Required tools

- Allen keys or bits 4-10 mm

- Screw bits and sockets

- Torx® keys or bits T6-T25

- Torque wrench

- Lifting device

- Screwdrivers

- Pliers

- Bearing puller (optional)

- Feeler gauge

Assembly

1. Fit a lifting eye in the rear end of the press, see dimensional drawings in ServAid.

2. Unscrew the screws in the front end of the press.

3. Lift the press to a vertical position.

4. Assemble the press to the mounting plate using new longer screws.

   See dimensional drawings in ServAid for the screw length.