# Vertical installation rear mounting

NOTICE

Do not let the press piston rod support the press weight during service or repairs.

Axial force on the PST press piston rod may completely damage the load cell.

Press | Rear mounted
--- | ---
PST 5 | M8 (8x)
PST10 | M8 (8x)
PST20 | M10 (8x)
PST35 | M10 (8x)
PST50 | M12 (8x)
PST100 | M16 (8x)

Required tools

- Allen keys or bits 4-10 mm

- Screw bits and sockets

- Torx® keys or bits T6-T25

- Torque wrench

- Lifting device

- Screwdrivers

- Pliers

- Bearing puller (optional)

- Feeler gauge

1. Use holes on both sides of the press when using rear screw holes

   Do not use too long screws, see dimensional drawings in ServAid.

2. Tighten the screws according to the Torque table .

   Make sure to support the press until all screws are tightened.