# Cleaning

Keep the MWR-25 TA clean.

After use, remove any traces of oil and grease from the MWR-25 TA with a soft cloth and a soft surface cleaner for oil/grease. Do not use aggressive or abrasive cleaner.

Use an anti-static cleaning cloth in order to remove dust from the MWR-25 TA.

Avoid using harsh detergents to clean the MWR-25 TA.

Clean the contact of the MWR-25 TA by using an electrical contact cleaner solution.