# Tightening Test

The Focus 61 sends the tightening program (Pset and Job) to the MWR-25 TA.

For more information on the configuration and the use of MWR-25 TA, refer to the Focus 61 User Guide.

When the MWR-25 TA receives the tightening program and the wrench is ready for use, the blue LED flashes.

Load the MWR-25 TA following the direction of the arrow as shown on the label on the MWR-25 TA body (see the figure below):

A | Blue LED | B | Tightening direction

During the measurement (MWR-25 TA is loaded with torque), the yellow LED flashes.

At the end of each tightening, the LEDs are alight according to the test result:

- Green LED: Tightening OK

- Red LED: Tightening NOT OK