# LEDs

The MWR-25 TA has three sets of LEDs and each set consists of red, green, yellow and blue LEDs.

A | LED | B | Right view
C | Left view | D | Top view

In the following, a description of the LEDs behavior.

If the MWR-25 TA is out from the MWR Charging cradle, the battery is charged and at least a job is available on the MWR-25 TA:

- Yellow LED blinks every 3 s and blue LED blinks every 1 s: the MWR-25 TA is ready to use and any force is applied.

- Green LED on for 3 s and blue LED blinks every 1 s: the last tightening is OK and any force is applied on the MWR-25 TA after click.

- Red LED on for 3 s and blue LED blinks every 1 s: the last tightening is NOK and any force is applied on the MWR-25 TA after click.

- Yellow LED blinks with an interval less than 1 s: the MWR-25 TA is measuring.

- Green LED on for 3 s, yellow LED on during deadtime and blue LED on after deadtime: the last tightening is OK (TOK) and any force is applied on MWR-25 TA after click.

- Red LED on for 3 s, yellow LED on during deadtime and blue LED on after deadtime: the last tightening is NOK (TNOK) and any force is applied on MWR-25 TA after click.

- Red LED on for 3 s, yellow LED on during deadtime and blue LED bliks every 1 s: the last tightening is rehit or NOK and any force is applied on MWR-25 TA after click.

If the MWR-25 TA is out from the MWR Charging cradle, the battery is out of power and at least, a job is available on the MWR-25 TA:

- Red LED blinks every 3 s and blue LED blinks every 1 s: the MWR-25 TA is ready to use.

- Green LED on for 3 s and blue LED blinks every 1 s: the last tightening is OK and any force is applied on the MWR-25 TA after click.

- Red LED on for 3 s and blue LED blinks every 1 s: the last tightening is NOK and any force is applied on the MWR-25 TA after click.

- Red LED blinks every 1 s: the MWR-25 TA is measuring.

- Green LED on for 3 s, yellow LED on during deadtime and blue LED on after deadtime: the last tightening is OK (TOK) and any force is applied on MWR-25 TA after click.

- Red LED on for 3 s, yellow LED on during deadtime and blue LED on after deadtime: the last tightening is NOK (TNOK) and any force is applied on MWR after click.

- Red LED on for 3 s, yellow LED on during deadtime and blue LED bliks every 1 s: the last tightening is rehit or NOK and any force is applied on MWR-25 TA after click.

If the MWR-25 TA is out from the Charging cradle, the battery is charged and no jobs are available on the MWR-25 TA:

- Yellow LED blinks every 3 s: theMWR-25 TA is ready to use and any force is applied.

- Red LED on for 3 s: the last tightening is OK and any force is applied on the MWR-25 TA after click.

- Red LED on for 3 s and blue LED blinks every 1 s: the last tightening is NOK and any force is applied on the MWR-25 TA after click.

- Yellow LED blinks with an interval less than 1 s: the MWR-25 TA is measuring.

If the MWR-25 TA is out from the MWR Charging cradle, the battery is out of power and no jobs are available on the MWR-25 TA:

- Red LED blinks every 3 s: the MWR-25 TA is ready to use and any force is applied.

- Red LED on for 3 s: the last tightening is OK and any force is applied on the MWR-25 TA after click.

- Red LED on for 3 s and blue LED blinks every 1 s: the last tightening is NOK and any force is applied on the MWR-25 TA after click.

- Red LED blinks every 1 s: the MWR-25 TA is measuring.

If the MWR-25 TA is in the MWR Charging cradle, the battery is charged and the MWR-25 TA is ready to use:

- Yellow LED on permanently and the blue LED blinks every 1 s: active job available on the MWR-25 TA.

- Yellow LED on permanently: no active job available on the MWR-25 TA.

If the MWR-25 TA is in the MWR Charging cradle, the battery is out of power and the MWR-25 TA is ready to use:

- Yellow LED on permanently and the blue LED blinks every 1 s: active job available on the MWR-25 TA.

- Yellow LED on permanently: no active job available on the MWR-25 TA.

If the MWR-25 TA is out the MWR Charging cradle and an error occurred: Red LED blinks every 300 ms

If the MWR-25 TA is in the MWR Charging cradle and an error occurred: Red LED blinks every 300 ms and yellow LED on permanently.

If the MWR-25 TA is out the MWR Charging cradle and it is out the radio range: Red LED, the green LED and the yellow LED blink every 3 s.

If the MWR-25 TA is in the Charging cradle and out of the radio range: Yellow LED blinks on permanently.