# Importing an ILT Base Station Configuration

A configuration from another ILT Base Station can be imported if needed.

1. Download the configuration to a USB drive.

   The configuration file must be placed at root level on the USB drive.

2. On the ILT Base Station, remove the lid protecting the USB port and connect the USB drive.

3. From the Home screen, select System, then select USB, and then select Import configuration.

4. Select the correct configuration.

   There can be several configuration files on one USB drive.

5. Select Yes to confirm the import of the new configuration. The ILT Base Station will restart after the transfer.

6. After the restart, remove the USB drive and close the lid protecting the USB port.

Relevant Information

- Exporting the ILT Base Station Configuration