# Exporting the ILT Base Station Configuration

A complete configuration backup for the ILT Base Station is created on the USB drive. This configuration file can be imported to another ILT Base Station or stored for later use.

1. On the ILT Base Station, remove the lid protecting the USB port and connect the USB drive.

2. From the Home screen, select System, then select USB, and then select Export configuration.
   The current configuration is saved to the USB drive.

3. A confirmation message will appear at the bottom of the screen after a successful export.

4. Remove the USB drive and close the lid protecting the USB port.

Relevant Information

- Importing an ILT Base Station Configuration