# Configuring the Controller Settings

When using an Ethernet connection, select Ethernet as connection type in the Controller connection menu. In Configure connection, the Power Focus controller IP and port are specified.

1. On the Home screen, select Configuration and then select Controller settings.

2. Select Connection type and then select one of the following options:

   - Ethernet, use this option when using an Ethernet connection.

   - RS232, use this option when using serial cable connection.

   - Offline, this option is only used for demonstration purposes and has no settings.

## Configuring the Ethernet settings

Entering the Power Focus IP

1. On the Controller settings screen, select Configure connection.

2. Select Power Focus IP, enter the correct IP number, and then select OK to confirm.

Entering the Power Focus Port

3. On the Controller settings screen, select Configure connection.

4. Select Power Focus Port, enter the correct Port number, and then select OK to confirm.

## Configuring the RS232 settings

Entering the Baud rate

1. On the Controller settings screen, select Configure connection.

2. Select Baud rate, enter the correct number, and then select OK to confirm.