# Power Supply

The ILT Base Station viewed from below

A | Ethernet, D-coded M12 female | B | Power I/O, 10-30 VDC ∼5 W, M8 male A-coded
C | USB type A, for USB drive | D | COM, RS-232, M8 female A-coded

Power is supplied to the ILT Base Station by 24 VDC through the connector marked “PWR”. It is recommended to connect the included power cable directly to the 24V and GND outputs on the Power Focus controller.

Make sure the Power Focus is turned off when connecting the ILT Base Station.

## Power (PWR) and Input/Output IO connector

Connector M8 Male A-coded

Pin | Wire color in the connected cable | Signal
--- | --- | ---
1 | Brown | +10-30 VCD in, ∼5 W
2 | White | Relay 1 Common Solid state relay, Galvanically isolated, 30V AC/DC, 1A, Internal resistance 0.15Ω
4 | Black | Relay 1 Normally open Solid state relay, Galvanically isolated, 30V AC/DC, 1A, Internal resistance 0.15Ω
3 | Blue | GND (System ground)

## RS-232 serial connector (COM)

Connector M8 Female A-coded

Connector M8 Female A-coded
Pin | Wire color in the connected cable | Signal
--- | --- | ---
1 | Brown | GND (System ground)
2 | White | RS-232 Tx
4 | Black | RS-232 Rx
3 | Blue | GND (System ground)