# Status LED behavior

Behavior | Color | Description
--- | --- | ---
Steady | Blue | MWR Charging Cradle is in stand-by mode (MWR out of the cradle)
Blinking with a 1 second interval | Green | MWR charging.
Steady | Green | MWR charge complete.
Steady | Red | Hardware error has occurred in MWR Charging Cradle.
Alternating | Red and blue | Conductance error has occurred while charging the MWR.

For more information about the MWR wrench's LEDs behavior while charging in the Cradle, refer to Charging the MWR with the MWR Charging Cradle.